Available 16-bit registers:		Available 32-bit registers: (386+)
AX	Accumulator			EAX
BX	Base register			EBX
CX	Counter				ECX
DX	Data register			EDX
SP	Stack pointer			ESP
BP	Base pointer			EBP
SI	Source index			ESI
DI	Destination index		EDI
DS	Data segment
ES	Extra segment
SS	Stack segment
CS	Code segment
FS	Extra segment 2 (386+)
GS	Extra segment 3 (386+)
IP	Instruction pointer		EIP
FL	Flags				EFL

Enter ?F to display the recognized flags.
