.TOPICLEN. 53
.MAXNUMHLP. 57
.HELPID. 1
.TOPICTEXT.Key Assignments Help
.HELPTEXT.       Key Assignments Help&
&
Enter    Places into memory the information&
         you select or type.&
&
Esc      Cancels the current screen and returns&
         you to the previous screen.  Information&
         on the current screen is not saved.&
&
Tab      Moves the selection cursor to the next&
         choice or entry on a screen.&
&
       Moves the cursor in the direction of the&
         arrow.&
&
F1       Displays help information.&
&
F3       Exits the SELECT program.  The information&
         you selected or typed is not saved.&

&
F9       Displays the key assignments and their&
         functions.&
.HELPTEND.


.HELPID. 2
.TOPICTEXT.Help Facility Help
.HELPTEXT. @             Help Facility Help
&
Help is available whenever F1=Help appears on a screen.
To get help for an item, highlight the item and press F1.&
&
From a help panel you can press the F9 key to view the
key assignments.@
.HELPTEND.


.HELPID. 3
.TOPICTEXT.Minimum DOS Function Help
.HELPTEXT. @            Minimum DOS Function Help
&
Select this option to allocate more memory for
running programs than for using DOS
functions.  This option is useful if you
use a large number of files or you calculate large
amounts of data.  Database and spreadsheet programs,
for example, require large amounts of memory.
Select this option if your system has 256K of memory
installed.@
.HELPTEND.


.HELPID. 4
.TOPICTEXT.Balance DOS Function Help
.HELPTEXT. @            Balance DOS Function Help
&
Select this option to balance the memory between the
DOS functions and the programs you use.
This option provides sufficient memory for programs
such as word processors or text editors.
Select this option if your system has 512K of memory installed.@
.HELPTEND.


.HELPID.  5
.TOPICTEXT.Maximum DOS Function Help
.HELPTEXT. @            Maximum DOS Function Help
&
Select this option if you want to allocate the
maximum amount of memory for DOS functions.&
Select this option if your system has more than
512K of memory installed.@
.HELPTEND.


.HELPID. 6
.TOPICTEXT.Accept Country and Keyboard Help
.HELPTEXT. @         Accept Country and Keyboard Help
&
Select this option to accept the country and
keyboard shown.  The SELECT program assigns
the appropriate monetary symbol, decimal
separator, date and time format, and keyboard
layout.@
.HELPTEND.


.HELPID. 7
.TOPICTEXT.Specify Country and Keyboard Help
.HELPTEXT. @        Specify Country and Keyboard Help
&
Select this option to choose a different country
and keyboard layout.@
.HELPTEND.


.HELPID. 8
.TOPICTEXT.Country Help
.HELPTEXT. @               Country Help
&
Use the Up or Down arrow keys to select a country,
then press Enter.  The SELECT program assigns the
appropriate monetary symbol, decimal separator,
and date and time format for the country.@
.HELPTEND.


.HELPID. 9
.TOPICTEXT.Keyboard Help
.HELPTEXT. @          Keyboard Help
&
Use the Up or Down arrow keys to select a keyboard,
then press Enter.&
&
Select "None" if you do not want to change the
keyboard layout.&
&
The SELECT program assigns the appropriate keyboard
layout.@
.HELPTEND.


.HELPID. 10
.TOPICTEXT.Keyboard Layout Help
.HELPTEXT. @                Keyboard Layout Help
&
The keyboard you selected has two versions.&
&
Use the Up or Down arrow key to select the
keyboard version you want, then press Enter.@
.HELPTEND.


.HELPID. 11
.TOPICTEXT.Installation Drive Help
.HELPTEXT.                Installation Drive Help
&
Use the Up or Down arrow key to select&
the drive you want to install DOS on,&
then press Enter.&
&
Option 1 installs DOS on a fixed disk,&
drive C.&
&
Option 2 installs DOS on a diskette.&
.HELPTEND.


.HELPID. 12
.TOPICTEXT.DOS Location Help
.HELPTEXT. @                 DOS Location Help
&
Accept or change the directory name shown.&
&
If you accept the directory name, DOS utilities
are placed in the DOS directory.&
&
If you change the directory name, DOS utilities
are placed in the directory you specify.
The directory name can have up to eight characters.
A backslash (\) must precede the directory name.&
&
Example :  C:\MINE&
&
           C:  specifies the drive and \MINE is&
               the new directory name.&
&
You can specify a directory path.  The directory path can
have up to 40 characters.  Use the backslash (\) to separate
the directory names in a path.
&
Example:  C:\DOS\DIR1\DIR2&
&
          C:  specifies the drive and&
          \DOS\DIR1\DIR2 is the directory path.@
.HELPTEND.


.HELPID. 13
.TOPICTEXT.Printer Selection Help
.HELPTEXT. @                 Printer Selection Help
&
Type in a number from 0 through 7 to show the number of
printers attached to your system.@
.HELPTEND.


.HELPID. 14
.TOPICTEXT.Printer Type Help
.HELPTEXT. @                 Printer Type Help
&
Use the Up or Down arrow keys to select the name of your
printer, then press Enter.  If the printer attached to your
system is not listed, select "Other" to identify the type
of printer you are using.  When more than one printer is
attached, this list reappears for each printer.
If you do not know the name or type of printer you have,
check the printer label or the manual that came with the
printer.@
.HELPTEND.



.HELPID. 15
.TOPICTEXT.Parallel Printer Port Help
.HELPTEXT. @            Parallel Printer Port Help
&
If you have one printer, press Enter to accept LPT1.&
&
If you have two printers, select LPT1 for your primary
printer and LPT2 for your secondary printer. If you
have three printers, select LPT3 for the third one.&
&
You can assign only one printer to each port.@
.HELPTEND.


.HELPID. 16
.TOPICTEXT.Serial Printer Port Help
.HELPTEXT. @            Serial Printer Port Help
&
If you have one printer, press Enter to accept COM1.&
&
If you have two printers, select COM1 for your primary
printer and COM2 for you secondary printer.  If you
have three printers, select COM3 for the third one.
If you have four printers, select COM4 for the fourth
printer.&
&
You can assign only one printer to each port.&
&
Note: Other devices, such as modems, lightpens, or a
mouse, attach to serial ports.  If you have one of these
devices, refer to the manual that came with the device
to determine which serial port to use.&
&
If you refer to your serial printer by a parallel port
name, press the Tab key to move to the options at the
bottom of the screen.@
.HELPTEND.


.HELPID. 17
.TOPICTEXT.Serial Printer/Parallel Port Help
.HELPTEXT. @       Serial Printer/Parallel Port Help
&
This option allows you to refer to your serial printer
as a parallel printer.  This option is useful if your
programs require that printer output be sent to a
parallel port.&
&
Select "None" if you use your printer only as a serial
printer.&
&
If you have one serial printer that you use as a
parallel printer select LPT1.&
&
If you have more than one serial printer that you
use as a parallel printer, select LPT 1 for your
primary printer, LPT2 for your secondary printer,
and LPT3 for your third printer.&
&
Do not select a parallel port for a serial printer if
that port has a parallel printer attached.@
.HELPTEND.


.HELPID. 18
.TOPICTEXT.Update DOS Files Help
.HELPTEXT. @            Update DOS Files Help
&
Select this option to replace previous DOS files.  This
option replaces previous DOS files in the directory specified, 
and installs the read-only system files in the root directory. &
&
This option does not replace DOS files in subdirectories
other than that specified.@
.HELPTEND.


.HELPID. 19
.TOPICTEXT.Update DOS Help
.HELPTEXT. @              Update DOS Help
&
Select this option to replace previous DOS files in the directory
you specify on drive C.  This option is useful if you want
DOS 4.0 to co-exist with a previous version of DOS or
another operating system, or when your system is a
network server.&
&
This option does not replace system files on an existing
system or DOS files in subdirectories across multiple
logical drives.&
&
For further information on replacing system files, refer to
the "MS-DOS 4.0 Users Guide" book.@
.HELPTEND.



.HELPID. 20
.TOPICTEXT.Continue Installation Help
.HELPTEXT. @            Continue Installation Help
&
Select this option to continue installing DOS without
reviewing the selections you made for your CONFIG.SYS
and AUTOEXEC.BAT files.@
.HELPTEND.


.HELPID. 21
.TOPICTEXT.Change Options Help
.HELPTEXT. @           Change Options Help
&
Select this option to review, change, or add values to
your CONFIG.SYS and AUTOEXEC.BAT files.&
&
Depending on the hardware installed on your system, you
can change or add options, such as expanded memory
support, FASTOPEN, and SHARE.&
&
When you change a selection from NO to YES, it increases
the amount of memory DOS uses.&
&
Refer to the "MS-DOS 4.0 Users Guide" book for additional
information.@
.HELPTEND.


.HELPID. 22
.TOPICTEXT.Code Page Switching Help
.HELPTEXT. @             Code Page Switching Help
&
Accept or change the choice shown.&
&
If you selected Denmark, Portugal, Norway,
or French-speaking Canada on a previous
display, set this choice to Yes.
&
Code Page Switching allows you
to change from one character set to
another so you can display or
print characters in different
languages.@
.HELPTEND.


.HELPID. 23
.TOPICTEXT.Expanded Memory Support Help
.HELPTEXT. @             Expanded Memory Support Help
&
Accept or change the choice shown.&
&
DOS uses expanded memory to hold part
of the operating system.  This provides
more memory for running programs that
require expanded memory support.&
&
Expanded Memory is available on the IBM
Personal System/2 (registered trademark of International
Business Machines) and on other IBM
PC/AT family and compatible computers with expanded 
memory cards.@
.HELPTEND.


.HELPID. 24
.TOPICTEXT.Extended Display Support Help
.HELPTEXT. @             Extended Display Support Help
&
Accept or change the choice shown.&
&
Extended display support (ANSI.SYS)
replaces the standard
input and output support on your
system.  ANSI.SYS provides extended
features, such as redefining keys,
manipulating the cursor, and displaying
color attributes.@
.HELPTEND.


.HELPID. 25
.TOPICTEXT.FASTOPEN Support Help
.HELPTEXT. @                  FASTOPEN Support Help
&
Accept or change the choice shown.&
&
FASTOPEN allows quick access to
recently opened files.@
.HELPTEND.


.HELPID. 26
.TOPICTEXT.GRAFTABL Display Support Help
.HELPTEXT. @             GRAFTABL Display Support Help
&
Accept or change the choice shown.&
&
GRAFTABL (Graphics Table) allows you
to display additional characters from
the National Language Code Page when
you use a color/graphics display adapter in
graphics mode.@
.HELPTEND.



.HELPID. 27
.TOPICTEXT.GRAPHICS Support Help
.HELPTEXT. @             GRAPHICS PrtSc Support Help
&
Accept or change the choice shown.&
&
GRAPHICS allows you to print the
contents of a graphics display.
This option prints graphics, such as
drawings, graphs, or charts.
Without GRAPHICS, you can print
text characters only.@
.HELPTEND.

.HELPID. 28
.TOPICTEXT.SHARE Support Help
.HELPTEXT. @             DOS SHARE Support Help
&
Accept or change the choice shown.&
&
SHARE provides support for file sharing and
diskette change protection.@
.HELPTEND.


.HELPID. 29
.TOPICTEXT.SHELL Support Help
.HELPTEXT. @             DOS SHELL Support Help
&
Accept or change the choice shown.&
&
The Shell program allows you to make selections
from menus instead of typing DOS commands.&
&
For additional information on the Shell program,
refer to the "MS-DOS 4.0 Users Guide"
book.@
.HELPTEND.


.HELPID. 30
.TOPICTEXT.Virtual Disk (RAMDRIVE) Support Help
.HELPTEXT. @             Virtual Disk Support Help
&
Accept or change the choice shown.&
&
RAMDRIVE allows you to use part of your
system memory to simulate a fixed disk
drive.  A virtual drive permits quick
access to files, but it is temporary,
and data stored on the virtual drive
is lost when you turn off the system.@
.HELPTEND.


.HELPID. 31
.TOPICTEXT.DOS PATH Help
.HELPTEXT. @                 DOS PATH Help
&
Accept or change the choice shown.&
&
DOS uses a path to search for files that
are not located in the current directory.&
DOS PATH searches only for files with the extensions
.COM, .EXE, or .BAT.  The (;) separates the pathnames.&
&
You can type up to 120 characters in this field.
If your typing scrolls out of view, use the right
or left arrow keys to see it.&
&
Example:  C:\DOS;C:\DIR1;C:\DIR2&
&
          PATH searches and locates files&
          in the DOS, DIR1, and DIR2&
          directories on drive C.@
.HELPTEND.


.HELPID. 32
.TOPICTEXT.APPEND Path Help
.HELPTEXT. @                 APPEND Path Help
&
Accept or change the choice shown.&
&
DOS uses a path to search for files that are
not in the current directory. APPEND searches
only for data files with extensions other than .COM,
.EXE, or .BAT.  The (;) separates the pathnames.&
&
You can type up to 120 characters in this field.
If your typing scrolls out of view, use the right
or left arrow keys to see it.&
&
Example:  C:\DOS;C:\DIR1;C:\DIR2&
&
          APPEND searches and locates files&
          in the DOS, DIR1, and DIR2&
          directories on drive C.@
.HELPTEND.


.HELPID. 33
.TOPICTEXT.PROMPT Help
.HELPTEXT. @                PROMPT Help
&
Accept or change the choice shown.&
&
Use the following list as a guide.  You can type
up to 120 characters in this field.  If your
typing scrolls out of view, use the right or
left arrow keys to see it.&
&
The default DOS prompt is C:\>.&
&
PROMPT entries :&
&
$B for the : character&
&
$D for the current date&
&
$E for the Esc character&
&
$G for the > character&
&
$H for backspace; the previous&
   character is erased&
&
$N for the current drive&
&
$P for the current directory&
&
$Q for the = character&
&
$T for the current time&
&
$V for the DOS version&
&
$1 for the < character&
&
$$ for the $ character&
&
$_ for advance a line&
&
Example:   C>prompt HELLO&
&
           Sets the DOS prompt to&
           the message HELLO.@
.HELPTEND.


.HELPID. 34
.TOPICTEXT.SHELL Parameters Help
.HELPTEXT. @           SHELL Parameters Help
&
Accept or change the choices shown.&
&
Use the following list as a guide.  You can type up
to 115 characters in this field.  If your typing
scrolls out of view, use the right or left arrow
keys to see it.&
&
The Shell program uses menus that allow you to make
selections instead of typing DOS commands.&
&
SHELL entries:&
&
 /B:xxx  Specifies a buffer size&
&
 /CLR:SHELL.CLR&
         Identifies the filename for the Shell&
         color setup.  SHELL.CLR is the default.&
&
 /CO1&
         Displays the Shell in 16-color,&
         high-resolution 640 x 350 graphics&
&
 /CO2&
         Displays the Shell in 2-color,&
         high resolution graphics&
&
 /CO3&
         Displays the Shell in 16-color,&
         high-resolution 640 x 480 graphics&
&
 /COLOR&
         Activates the "Change colors" option&
&
 /COM2&
        Identifies a serial mouse installed on the&
        second serial port (installation default&
        is COM1)&
&
 /DATE&
         Displays the date and time&
&
 /DOS&
         Activates the File System in the Shell&
&
 /EXIT&
         Activates the "Exit Shell" option&
&
 /LF&
         Enables a mouse for left-handed use&
&
 /MAINT&
         Activates the ability to do&
         maintenance in Start Programs&
&
 /MENU&
         Activates the Start Programs in the&
         Shell&
&
 /MEU:SHELL.MEU&
         Identifies the filename of the Main Group&
         structure for the Start Programs&
&
 /MOS:PCIBMDRV.MOS&
        Identifies the filename of the IBM mouse&
        driver&
&
 /MOS:PCMSDRV.MOS&
        Identifies the filename of the Microsoft&
        serial mouse driver&
&
 /MOS:PCMSPDRV.MOS&
        Identifies the filename of the Microsoft&
        parallel mouse driver&
&
 /MUL&
        Provides multiple directory and file&
        buffers in the File System&
&
 /PROMPT&
        Activates the Shell command prompt&
&
 /SND&
        Enables the speaker for sound&
&
 /SWAP&
        Activates saving (swapping) files and&
        directories to a disk file while&
        performing tasks at the Shell command&
        prompt&
&
 /TEXT&
        Displays the Shell in text mode&
&
 /TRAN&
        Operates the Shell in transient mode@
.HELPTEND.


.HELPID. 35
.TOPICTEXT.FASTOPEN Parameters Help
.HELPTEXT. @            FASTOPEN Parameters Help
&
Accept or change the choice shown.&
&
Use the following list as a guide.  You can type
up to 60 characters in this field.  If your typing
scrolls out of view, use the left or right arrow
keys to see it.&
&
FASTOPEN allows quick access to recently
opened files.&
&
FASTOPEN entries:&
&
C:&
           Specifies the drive&
&
N = 10 to 999&
           Specifies the number of directories or&
           file entry buffers allocated in memory&
&
M = 1 to 999&
           Specifies the number of continuous&
           space buffers allocated in memory&
&
/X&
           Used when expanded memory support is&
           available.  When using the /X option&
           the value of "N" or "M" should not&
           exceed 150.&
&
Example:  C:=(50,25)&
&
          Specifies FASTOPEN on drive C with&
          50 file and directory entry buffers and&
          25 continuous space buffers.@
.HELPTEND.


.HELPID. 36
.TOPICTEXT.SHARE Parameters Help
.HELPTEXT. @             SHARE Parameters Help
&
Accept or change the choice shown.&&
Use the following list as a guide.&
&
SHARE provides support for file sharing and
diskette change protection.&
&
SHARE Parameters:&
&
 /F:     Allocates file space in bytes for the&
         area used to record information for file&
         sharing&
&
 /L:     Allocates space for the number of locks&
         you want.  Lock denies read/write access&
         to regions of a file.&
&
Example: /F:2048 /L:20&
&
         Specifies a filespace of 2048 bytes and&
         20 locks.@
.HELPTEND.


.HELPID. 37
.TOPICTEXT.GRAPHICS Parameters Help
.HELPTEXT. @           GRAPHICS Parameters Help
&
Accept or change the choice shown.&
&
Use the following list as a guide.  You can type
up to 80 characters in this field.  If your typing
scrolls out of view, use the left or right arrow
keys to see it.&
&
GRAPHICS prints the contents of a graphics display.
This is useful, if you print charts, tables, or
drawings.&
&
GRAPHICS Parameters:&
&
 COLOR1&
          IBM 5182 Color Printer with black ribbon&
&
 COLOR4&
          IBM 5182 Color Printer with red, green,&
          blue, and black ribbon&
&
 COLOR8&
          IBM 5182 Color Printer with black, cyan,&
          magenta, and yellow ribbon&
&
 GRAPHICS&
          IBM 5152 Graphics Printer&
          IBM Proprinters&
          IBM 3812 Pageprinter&
          IBM 5202 Quietwriter (registered&
          trademark of International Business&
          Machines) III Printer&
          IBM 5204 Quickwriter (trademark of&
          International Business Machines) Printer&
&
 GRAPHICSWIDE&
          IBM 5152 Graphics Printer&
          IBM Proprinters (both are set for wide&
          paper)&
&
 THERMAL&
         IBM 5140 Convertible Printer&
&
 /B&
         Specifies background color printing for&
         COLOR4 and COLOR8 printers&
&
 /LCD&
         Prints data as it appears on a liquid&
         crystal display&
&
 /R&
         Prints black and white as it appears on&
         the display&
&
Example: COLOR8 /B/R&
&
         Specifies black, white, and background&
         color printing for the 5182 Color Printer.&
&
 /PB:ID&
         Prints data using the print box size&
         specified by the ID.  The ID should match&
         the first operand of a Printbox statement&
         in the printer profile.  You may use&
         /PRINTBOX:ID in place of /PB:ID.&
&
Supported IDS:&
&
LCD&
         Specifies the LCD printbox.  When used&
         with an LCD display, the data is printed&
         as it appears on the LCD display.&
         This entry has the same effect as /LCD.&
&
STD&
         Specifies standard printbox, which is the&
         default value.@
.HELPTEND.


.HELPID. 38
.TOPICTEXT.XMAEM Parameters Help
.HELPTEXT. @            XMAEM Parameters Help
&
Accept or change the choice shown.  Type, in 16KB
increments, the amount of memory you want to allocate.
If you do not specify an amount, the system allocates
all memory above 1MB.&
&
XMAEM enables your system to access the extended memory
available as expanded memory.&
&
Example:  DEVICE=XMAEM.SYS 64&
&
          Allocates 1 megabyte of extended memory.&
&
For additional information, refer
to the "MS-DOS 4.0 Users Guide" book.@
.HELPTEND.


.HELPID. 39
.TOPICTEXT.XMA2EMS Parameters Help
.HELPTEXT. @            XMA2EMS Parameters Help
&
Accept or change the choice shown.  If you change
the segment address values, you must
define unused 64KB contiguous space for the FRAME and
unused 16KB contiguous space for the Pxxx pages.&
&
Example:  FRAME=D000 P254=C000 P255=C400&
&
Note:  These values are sample defaults only and&
       may not reflect actual free segments in your&
       system.&
&
For additional information, refer to the "MS-DOS 4.0
Users Guide" book.@
.HELPTEND.


.HELPID. 40
.TOPICTEXT.RAMDRIVE Parameters Help
.HELPTEXT. @         RAMDRIVE Parameters Help
&
Accept or change the choice shown.  Use the
following list as a guide.&
&
RAMDRIVE allows you to use part of the system
memory to simulate a fixed disk drive.  A
virtual drive permits quick access to files,
but it is temporary, and data stored on a
virtual drive is lost when you turn off
the system.&
&
RAMDRIVE Parameters:&
&
 Buffer:&
       Buffer size in kilobytes;&
       16KB is the minimum buffer size&
&
 Sector:&
       Sector size in bytes;&
       128, 256, 512, or 1024 bytes&
&
 Directory entries:&
       Number of root directory entries;&
       3 to 1024&
&
 /E&
       Used when extended memory support&
       is available&
&
 /A&
       Used when expanded memory support&
       is available&
&
Example:  160 512 64&
&
          Specifies the size of the buffers,&
          sectors, and the number of directories.@
.HELPTEND.


.HELPID. 41
.TOPICTEXT.BREAK Help
.HELPTEXT.             BREAK (Control Break) Help
&
Accept or change the choice shown.&
&
ON:   DOS always checks for a Ctrl+Break key&
      sequence and permits input or output to&
      a device to be canceled.&
&
OFF:  DOS checks for a Ctrl+Break key sequence only&
      during standard input, output, print, and&
      auxiliary device operations.&
.HELPTEND.


.HELPID. 42
.TOPICTEXT.BUFFERS Help
.HELPTEXT. @                BUFFERS Help
&
Accept or change the choice shown.  Use the
following list as a guide.&
&
The value shown specifies the number of disk buffers
DOS allocates in memory.  If a second value is shown,
this value specifies the number of sectors the system
can read or write when processing an input or output
operation.&
&
If you do not specify a buffer, DOS sets a value
based on the amount of system memory.&
&
BUFFERS Values:&
&
1 to 99       Number of buffers the system uses&
&
1 to 8        Number of sectors the system can&
              read or write in processing an input&
              or output operation@
.HELPTEND.


.HELPID. 43
.TOPICTEXT.APPEND Parameter Help
.HELPTEXT. @            APPEND Parameter Help
&
Accept or change the choice shown.  Use the
following list as a guide.&
&
APPEND locates data files outside of the current
directory that have extensions other then .COM,
.EXE, or .BAT.&
&
APPEND Parameters:&
&
/X:ON or /X&
         Tells APPEND to search and process&
         executable files&
&
 /X:OFF (default value)&
         Tells APPEND not to search and&
         process executable files.&
&
/PATH:ON (default value)&
         Tells APPEND to search for files that have&
         a drive or a path specified&
&
/PATH:OFF&
         Tells APPEND not to search for files that&
         have a drive or a path specified&
&
/E&
         Keeps the APPEND paths in the DOS&
         environment.  APPEND searches the&
         environment on each call to find the path.&
&
;&
         Separates the APPEND paths, or cancels the&
         APPEND paths if the semi-colon is the only&
         parameter used.&
&
Example: /E /X&
         APPEND is in the DOS environment&
         where it searches and processes&
         executable files with extensions of&
         .COM, .EXE, or .BAT.@
.HELPTEND.


.HELPID. 44
.TOPICTEXT.FCBS Help
.HELPTEXT. @                 FCBS Help
&
Accept or change the choice shown.  Use the
following list as a guide.&
&
FCBS allows you to specify the number of file
control blocks that DOS can open concurrently.&
&
FCBS Values:&
&
 1 to 255   Number of file control blocks&
&
 0 to 255   Number of protected file control blocks&
&
Example:  20,10&
&
          Specifies 20 FCBS open and 10 protected&
          from being automatically closed by DOS.@
.HELPTEND.


.HELPID. 45
.TOPICTEXT.FILES Help
.HELPTEXT. @                 FILES Help
&
Accept or change the choice shown.&
&
If you do not specify a value, DOS uses a value of 8.&
&
The value specifies the number of files that&
can be open at any one time.  The value can be&
from 8 through 255.@
.HELPTEND.


.HELPID. 46
.TOPICTEXT.LASTDRIVE Help
.HELPTEXT. @                 LASTDRIVE Help
&
Accept or change the choice shown.&
&
If you do not specify a value, DOS uses a value of E.&
&
This value identifies the last drive installed on
your system.  The value can be a letter from A through
Z, and it must represent the last valid drive letter
that DOS can accept.@
.HELPTEND.


.HELPID. 47
.TOPICTEXT.STACKS Help
.HELPTEXT. @                 STACKS Help
&
Accept or change the choice shown.&
&
This value (if any) specifies stack resources.
Use the following list as a guide.  You must
specify a number for each frame and a size,
in bytes, for each frame.&
&
STACKS Values:&
&
8  to 64    Number of stack frames&
&
32 to 512   Size of each stack frame&
&
Example:  8 128&
&
          Specifies 8 stack frames of 128 bytes&
          each.@
.HELPTEND.


.HELPID. 48
.TOPICTEXT.VERIFY Help
.HELPTEXT. @                VERIFY Help
&
Accept or change the choice shown.&
&
VERIFY confirms that data is correctly
written to a disk.&
&
ON:   DOS confirms the data can be read&
      without error.&
&
OFF:  DOS does not verify the data.@
.HELPTEND.


.HELPID. 49
.TOPICTEXT.Use SELECT Partition Sizes Help
.HELPTEXT. @           Use SELECT Partition Sizes Help
&
Select this option to partition your fixed
disk into one partition.&
&
Note:  If you have a Personal System/2 with a&
       partition greater than 32MB and want to&
       install a keyboard password, refer to the&
       "MS-DOS 4.0 Users Guide" book for&
       additional information.@
.HELPTEND.


.HELPID. 50
.TOPICTEXT.Define Your Own Partitions Sizes Help
.HELPTEXT. @      Define Your Own Partitions Sizes Help
&
Select this option if you want to use FDISK to partition
your fixed disk.&
&
Note:  If you have a Personal System/2 with a&
       partition greater than 32MB and want to&
       install a keyboard password, refer to the&
       "MS-DOS 4.0 Users Guide" book for&
       additional information.@
.HELPTEND.


.HELPID. 51
.TOPICTEXT.Leave Disk Unchanged Help
.HELPTEXT. @          Leave Disk Unchanged Help
&
Select this option if you do not want to change
the non-allocated partition space on your fixed disk.@
.HELPTEND.


.HELPID. 52
.TOPICTEXT.Define Your Own Sizes Help
.HELPTEXT. @           Define Your Own Sizes Help
&
Select this option if you want to partition the non-allocated
space on your fixed disk.  Refer to the "MS-DOS 4.0 Users
Guide" book for information on using FDISK.@
.HELPTEND.

.HELPID. 53
.TOPICTEXT.Date and Time Help
.HELPTEXT. @                 Date and Time Help
&
Type the date and time in the fields provided.  The system clock
keeps an accurate record of the date and time.@
.HELPTEND.


.HELPID. 54
.TOPICTEXT.Format Fixed Disk Help
.HELPTEXT. @           Format Fixed Disk Help
&
Select this option to format your fixed disk.
A partition must be formatted before data can
be placed on it.&
&
Warning :
If your fixed disk is already formatted, this option will
reformat the disk and destroy all information on
the disk.  Refer to the "MS-DOS 4.0 Users Guide"
book for additional information.@
.HELPTEND.


.HELPID. 55
.TOPICTEXT.Do Not Format Fixed Disk Help
.HELPTEXT. @       Do Not Format Fixed Disk Help
&
Select this option if you do not want to format
your fixed disk.@
.HELPTEND.


.HELPID. 56
.TOPICTEXT.Install the MS-DOS Shell Help
.HELPTEXT. @           Install the MS-DOS Shell Help
&
Select this option if you want the MS-DOS Shell
to be installed by SELECT onto the target system.&
&
The MS-DOS Shell lets you choose options from
menus instead of typing DOS commands.@
.HELPTEND.


.HELPID. 57
.TOPICTEXT.Do not install the MS-DOS Shell Help
.HELPTEXT. @       Do not install the MS-DOS Shell Help
&
Select this option if you do not want the MS-DOS 
Shell to be installed by SELECT onto the target 
system.@
.HELPTEND.
